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Overview

The newest addition to the Solutionz RMM “V” series Vaults, the V1610, features the Intel® Pentium® Silver N6005 processor with 16GB soldered (fixed) DDR4 memory and 32GB onboard eMMC. It also includes three additional M.2 slots for optional NVMe SSD storage, WiFi, and LTE modules. The V1610 is equipped with six Intel® I226-V RJ-45 Ethernet ports, supporting up to 2.5 Gigabit ethernet connectivity with backwards compatibility. 

The operating system is Ubuntu 24.04.3, custombuilt and performanceoptimized to seamlessly support the Solutionz RMM Platform. 

Protectli Vaults utilize Intel components ensuring persistent compatibility with a wide range of operating systems (OS) and applications. The "V" series Vaults feature a fanless, all-aluminum chassis design, allowing for efficient heat dissipation from the CPU and other components without any moving parts or additional power requirements.

Technical Specifications

	Model 
	V1610 

	Description 
	6x 2.5G Network Port Fanless Appliance 

	Processor 
	Intel® Pentium® Silver N6005 (64 Bit, 2.0GHz, Turbo 3.3GHz, 4M L3 Cache) 

	Processor Cores 
	4 

	Processor Threads 
	4 

	Processor Capabilities 
	AES-NI 

	
	Intel® Vt-x, Vt-d 

	Network 
	6x Intel® I226-V 2.5G Ethernet, RJ-45 

	Video / Graphics 
	Intel® UHD Graphics, 1x HDMI 2.0 

	Audio 
	Audio over HDMI 

	Memory 
	1x 16GB LPDDR4-2933, Soldered 

	Operating System 
	Linux - Ubuntu 24.04.3 LTS (minimized CLI version) 
 

	Chassis 
	Fanless, Aluminum, Gray 

	 
Chassis Dimensions 
	w/ feet: 5.6 x 4.8 x 2.3in. (142.1 x 121.0 x 57.7mm) 
w/o feet: 5.6 x 4.8 x 2.1in. (142.1 x 121.0 x 55.1mm) 






External Interfaces

Front Panel Configuration
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	Item # 
	Object 
	Label 
	Description 

	1 
	Reset Button (Recessed) 
	RESET 
	An ACPI reset button. 

	2 
	Power Button 
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	Pressing the Power Button will power the unit on an illuminate with a blue LED. 
In OSes configured to handle ACPI signals, pressing the power button initiates a shutdown. 
Pressing and holding the Power Button for 5 seconds will force the unit to power off. 

	3 
	USB Type-A Ports 
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	Four USB 3.2 Gen 1† Type-A ports. (Maximum theoretical throughput of 5000Mbps [~500MBps]) 

	4 
	HDMI Port 
	HDMI 
	Video and audio output via HDMI 2.0 port. 

	5
	Onboard Micro (3FF) SIM Slot
	SIM
	Access to an onboard Micro (3FF) SIM slot for providing a SIM card to an optional internal cellular modem.




Rear Panel Configuration
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	Item # 
	Object 
	Label 
	Description 

	1 
	Power Supply Connector 
	 
 
	12V DC locking collar connector for the included 48W external power supply. Positive rail is the tip, negative is sleeve. 
Barrel dimensions: 5.5mm x 2.5mm 

	2 
	Ethernet Ports 
	1, 2, 3, 4, 5, 
6 
	Six (6) 10/100/1000/2500 Mbps Intel® I226-V ethernet ports. Ports 1, 2, and 3 are behind a PCIe switch (ASM2806). LEDs on the right side of NIC emit solid green when connected at any speed. 

	3 
	Type-C Serial Console Port 
	COM 
	RS-232 serial communications via FTDI FT232RQ UART, exposed through USB 2.0 Type C connector. Default port settings: 
· 115200 baud 
· No parity 
· 8 databits 
· 1 stopbit 

	4 
	Power Indicator LED 
	 
 
	LED emits solid green when the device is powered on. 

	5 
	Data Activity LED 
	 
 
	LED emits red when data activity is detected over the NVMe interface. 



Dimension View [image: ]

image10.png




image11.png




image12.png
Ss-T.-




image13.png




image14.png




image15.png




image16.png




image17.png
2.3in. (57.7mm)

PROTECTLI

)

E
E
N
<

(

5.6in.





image7.png
SOLUTIONZ




image1.png




image2.png




image4.png




image5.png




image3.png
7T





image6.png




image8.png
7T





image9.png




